 **2017 ANNUAL**  
 **INSPECTOR’S FORM**

THIS FORM IS TO BE COMPLETED ONLY BY AN AUTHORIZED SONOMA DRIFT TECH CENTER OR AUTHORIZED SONOMA DRIFT TECH PERSONNEL DURING ANNUAL INSPECTION.  
*Note: Not all items applicable to all classes of vehicles. A number of items are not required*

RULE BOOK / TECH DISCLAIMERThe rules and/or tech regulations set forth herein are designed to provide for the orderly conduct of racing events and to establish minimum acceptable requirements for such events. These rules shall govern the condition . of all events, and by participating in these events, all participants are deemed to have complied with these rules. **NO EXPRESSED OR IMPLIED WARRANTY OF SAFETY SHALL RESULT FROM . PUBLICATIONS OF OR COMPLIANCE WITH THESE RULES ANDIOR REGULATIONS.** They are intended as a guide for the conduct of the sport and are in no way a guarantee against injury or death to a participant, spectator, tech official or official.

The race director shall be empowered to permit reasonable and appropriate deviation from any of the specifications herein or impose any further restrictions that in his opinion do not alter the minimum acceptable requirements. **NO EXPRESSED OR IMPLIED WARRANTY OF SAFETY SHALL RESULT FROM SUCH ALTERATION OF SPECIFICATIONS.**

Any interpretation or deviation of these rules is left to the discretion of the officials. Their decision is final.

**VEHICLE EXTERIOR**\_\_ Crash bar or factory bumper required on front end  
\_\_ Tow hooks, front and rear  
\_\_ No sharp edges  
  
**ENGINE COMPARTMENT**  
\_\_ Clean  
\_\_ Coolant overflow  
\_\_ Oil overflow  
\_\_ No fluid leaks  
\_\_ Battery secured  
\_\_ Battery positive terminal covered  
\_\_ Batteries in driver’s compartment needs to be in a sealed box (unless the battery is dry cell type)  
\_\_ Starter positive terminal covered  
\_\_ No loose wires  
\_\_ Condition of hoses  
\_\_ No firewall holes  
\_\_ Brake fluid level/condition  
\_\_ Engine mounts  
\_\_ Operation of hood release/pins

**ROLL CAGE**\_\_ Cage number stamped \_\_\_\_\_  
\_\_ Main hoop 1 piece, 4 bends max  
\_\_ Rear down tubes not bent  
\_\_ Door bars  
\_\_ Diagonal bar  
\_\_ All mandrel bends  
\_\_ Mounting plates  
\_\_ 360 welds on required bars  
\_\_ General condition  
\_\_ Padding on contact areas  
\_\_ Broomstick test – open cars

**HAND EXTINGUISHER**  
\_\_ Within driver’s reach  
\_\_ 2lb minimum ABC, full  
\_\_ Metal mounting plate/bracket  
\_\_ Mounting bracket bolted in

**DRIVER COMPARTMENT**  
\_\_ If fuel cell is located in driver compartment, a fire wall is required  
\_\_ Electrical cutoff switch function  
\_\_ Cutoff switch terminals covered  
\_\_ No sharp edges

**DRIVER SEAT**  
\_\_ Factory seat or better  
\_\_ Mounted securely

**HARNESS**  
\_\_ Mounting points  
\_\_ Condition of webbing  
\_\_ Shoulder belt mounting no more  
 than 20 degrees from horizontal  
\_\_ Lap belt mounting  
 **DRIVER EMERGENCY EXIT TIME**  
\_\_ Exit within 10 seconds starting  
 in as-raced condition through door  
  
**STEERING AND SUSPENSION**\_\_ No significant play in steering, bearings or suspension  
\_\_ If keyless start column lock is removed

Season annual valid for: \_\_\_\_\_\_\_\_  
  
Inspector Name Vehicle Log Book Number

Signature or Shop Stamp: Date: